Cmp-Mod V01 Created by CvPcb (2012-apr-16-27)-stable date = Wed 02 Oct 2013 18:49:54 BST

BeginCmp
TimeStamp = /523EF259;
Reference = C1;
ValeurCmp = 22pF;
IdModule  = C1;
EndCmp

BeginCmp
TimeStamp = /523EFED8;
Reference = C2;
ValeurCmp = 100nF;
IdModule  = C1;
EndCmp

BeginCmp
TimeStamp = /523EF260;
Reference = C3;
ValeurCmp = 22pF;
IdModule  = C1;
EndCmp

BeginCmp
TimeStamp = /523EF28C;
Reference = C4;
ValeurCmp = 10uF;
IdModule  = C1V5;
EndCmp

BeginCmp
TimeStamp = /524054F1;
Reference = C5;
ValeurCmp = 100nF;
IdModule  = C1;
EndCmp

BeginCmp
TimeStamp = /523F03DB;
Reference = C6;
ValeurCmp = 100nF;
IdModule  = C1;
EndCmp

BeginCmp
TimeStamp = /523F03E6;
Reference = C7;
ValeurCmp = 4.7uF;
IdModule  = C1;
EndCmp

BeginCmp
TimeStamp = /523F03E2;
Reference = C8;
ValeurCmp = 100nF;
IdModule  = C1;
EndCmp

BeginCmp
TimeStamp = /523F03F0;
Reference = C9;
ValeurCmp = 47pF;
IdModule  = C1;
EndCmp

BeginCmp
TimeStamp = /523F03E9;
Reference = C10;
ValeurCmp = 47pF;
IdModule  = C1;
EndCmp

BeginCmp
TimeStamp = /523F03EE;
Reference = C11;
ValeurCmp = 100nF;
IdModule  = C1;
EndCmp

BeginCmp
TimeStamp = /524059E3;
Reference = C12;
ValeurCmp = 10uF;
IdModule  = C1;
EndCmp

BeginCmp
TimeStamp = /524059E7;
Reference = C13;
ValeurCmp = 100nF;
IdModule  = C1;
EndCmp

BeginCmp
TimeStamp = /524059F9;
Reference = C14;
ValeurCmp = 10uF;
IdModule  = C1V5;
EndCmp

BeginCmp
TimeStamp = /52405A99;
Reference = C15;
ValeurCmp = 100uF;
IdModule  = C1V7;
EndCmp

BeginCmp
TimeStamp = /52405A9D;
Reference = C16;
ValeurCmp = 100uF;
IdModule  = C1V7;
EndCmp

BeginCmp
TimeStamp = /52405A8D;
Reference = C17;
ValeurCmp = 100uF;
IdModule  = C1V7;
EndCmp

BeginCmp
TimeStamp = /5242CA9A;
Reference = D1;
ValeurCmp = DIODE;
IdModule  = D4;
EndCmp

BeginCmp
TimeStamp = /5242CAA5;
Reference = D2;
ValeurCmp = DIODE;
IdModule  = D4;
EndCmp

BeginCmp
TimeStamp = /523EF16D;
Reference = IC1;
ValeurCmp = ATMEGA1284-P;
IdModule  = DIP-40__600_ELL;
EndCmp

BeginCmp
TimeStamp = /524586E7;
Reference = J1;
ValeurCmp = USB_2_UPDATE;
IdModule  = USB_B;
EndCmp

BeginCmp
TimeStamp = /523EFF8C;
Reference = K1;
ValeurCmp = X_MIN;
IdModule  = PIN_ARRAY_3X1;
EndCmp

BeginCmp
TimeStamp = /523EFF92;
Reference = K2;
ValeurCmp = X_MAX;
IdModule  = PIN_ARRAY_3X1;
EndCmp

BeginCmp
TimeStamp = /523EFF98;
Reference = K3;
ValeurCmp = Y_MIN;
IdModule  = PIN_ARRAY_3X1;
EndCmp

BeginCmp
TimeStamp = /523EFFE8;
Reference = K4;
ValeurCmp = Y_MAX;
IdModule  = PIN_ARRAY_3X1;
EndCmp

BeginCmp
TimeStamp = /523EFFED;
Reference = K5;
ValeurCmp = Z_MIN;
IdModule  = PIN_ARRAY_3X1;
EndCmp

BeginCmp
TimeStamp = /523EFFF6;
Reference = K6;
ValeurCmp = Z_MAX;
IdModule  = PIN_ARRAY_3X1;
EndCmp

BeginCmp
TimeStamp = /5242C8F1;
Reference = K7;
ValeurCmp = RELAY_2RT;
IdModule  = relay_2rt_l;
EndCmp

BeginCmp
TimeStamp = /5242C952;
Reference = K8;
ValeurCmp = RELAY_2RT;
IdModule  = relay_2rt_l;
EndCmp

BeginCmp
TimeStamp = /523EFC3F;
Reference = P1;
ValeurCmp = ISP;
IdModule  = pin_array_3x2;
EndCmp

BeginCmp
TimeStamp = /52405821;
Reference = P2;
ValeurCmp = M1_IN;
IdModule  = bornier2;
EndCmp

BeginCmp
TimeStamp = /52405829;
Reference = P3;
ValeurCmp = M1_OUT;
IdModule  = bornier2;
EndCmp

BeginCmp
TimeStamp = /524056D4;
Reference = P4;
ValeurCmp = M2_IN;
IdModule  = bornier2;
EndCmp

BeginCmp
TimeStamp = /524056DD;
Reference = P5;
ValeurCmp = M2_OUT;
IdModule  = bornier2;
EndCmp

BeginCmp
TimeStamp = /52404DD3;
Reference = P6;
ValeurCmp = X_AXIS;
IdModule  = bornier4;
EndCmp

BeginCmp
TimeStamp = /52404DE1;
Reference = P7;
ValeurCmp = Y_AXIS;
IdModule  = bornier4;
EndCmp

BeginCmp
TimeStamp = /52404DF7;
Reference = P8;
ValeurCmp = Z_AXIS;
IdModule  = bornier4;
EndCmp

BeginCmp
TimeStamp = /52404DB9;
Reference = P9;
ValeurCmp = CONN_4;
IdModule  = PIN_ARRAY_4x1;
EndCmp

BeginCmp
TimeStamp = /52404DDB;
Reference = P10;
ValeurCmp = CONN_4;
IdModule  = PIN_ARRAY_4x1;
EndCmp

BeginCmp
TimeStamp = /52404DF1;
Reference = P11;
ValeurCmp = CONN_4;
IdModule  = PIN_ARRAY_4x1;
EndCmp

BeginCmp
TimeStamp = /52404B5F;
Reference = P12;
ValeurCmp = CONN_8;
IdModule  = SIL-8;
EndCmp

BeginCmp
TimeStamp = /52404B6B;
Reference = P13;
ValeurCmp = CONN_8;
IdModule  = SIL-8;
EndCmp

BeginCmp
TimeStamp = /52404B70;
Reference = P14;
ValeurCmp = CONN_8;
IdModule  = SIL-8;
EndCmp

BeginCmp
TimeStamp = /52404B7F;
Reference = P15;
ValeurCmp = CONN_8;
IdModule  = SIL-8;
EndCmp

BeginCmp
TimeStamp = /52404B84;
Reference = P16;
ValeurCmp = CONN_8;
IdModule  = SIL-8;
EndCmp

BeginCmp
TimeStamp = /52404B88;
Reference = P17;
ValeurCmp = CONN_8;
IdModule  = SIL-8;
EndCmp

BeginCmp
TimeStamp = /52404BE1;
Reference = P18;
ValeurCmp = CONN_3X2;
IdModule  = pin_array_3x2;
EndCmp

BeginCmp
TimeStamp = /52404C6F;
Reference = P19;
ValeurCmp = CONN_3X2;
IdModule  = pin_array_3x2;
EndCmp

BeginCmp
TimeStamp = /52404C7E;
Reference = P20;
ValeurCmp = CONN_3X2;
IdModule  = pin_array_3x2;
EndCmp

BeginCmp
TimeStamp = /52405BBF;
Reference = P21;
ValeurCmp = M_PWR;
IdModule  = bornier2;
EndCmp

BeginCmp
TimeStamp = /524079A6;
Reference = P22;
ValeurCmp = PIN_HEADER;
IdModule  = SIL-7;
EndCmp

BeginCmp
TimeStamp = /524077B1;
Reference = P23;
ValeurCmp = I2C;
IdModule  = PIN_ARRAY_4x1;
EndCmp

BeginCmp
TimeStamp = /524078FF;
Reference = P24;
ValeurCmp = Z_PROBE;
IdModule  = bornier2;
EndCmp

BeginCmp
TimeStamp = /5242C779;
Reference = P25;
ValeurCmp = 12Volts;
IdModule  = bornier2;
EndCmp

BeginCmp
TimeStamp = /5242C77C;
Reference = P26;
ValeurCmp = 5Volts;
IdModule  = bornier2;
EndCmp

BeginCmp
TimeStamp = /5242CA38;
Reference = P27;
ValeurCmp = R1_IN;
IdModule  = bornier2;
EndCmp

BeginCmp
TimeStamp = /5242CA5A;
Reference = P28;
ValeurCmp = R2_IN;
IdModule  = bornier2;
EndCmp

BeginCmp
TimeStamp = /5242CA1D;
Reference = P29;
ValeurCmp = R1_OUT;
IdModule  = bornier2;
EndCmp

BeginCmp
TimeStamp = /5242CA43;
Reference = P30;
ValeurCmp = R2_OUT;
IdModule  = bornier2;
EndCmp

BeginCmp
TimeStamp = /5245890E;
Reference = P31;
ValeurCmp = MOUNT;
IdModule  = 1pin;
EndCmp

BeginCmp
TimeStamp = /52458919;
Reference = P32;
ValeurCmp = MOUNT;
IdModule  = 1pin;
EndCmp

BeginCmp
TimeStamp = /5245891D;
Reference = P33;
ValeurCmp = MOUNT;
IdModule  = 1pin;
EndCmp

BeginCmp
TimeStamp = /52458921;
Reference = P34;
ValeurCmp = MOUNT;
IdModule  = 1pin;
EndCmp

BeginCmp
TimeStamp = /5240582E;
Reference = Q1;
ValeurCmp = MOSFET_N;
IdModule  = TO220_VERT_MOSFET;
EndCmp

BeginCmp
TimeStamp = /5240564A;
Reference = Q2;
ValeurCmp = MOSFET_N;
IdModule  = TO220_VERT_MOSFET;
EndCmp

BeginCmp
TimeStamp = /5242CC41;
Reference = Q3;
ValeurCmp = PN2222A;
IdModule  = TO92;
EndCmp

BeginCmp
TimeStamp = /5242CC4A;
Reference = Q4;
ValeurCmp = PN2222A;
IdModule  = TO92;
EndCmp

BeginCmp
TimeStamp = /523EF471;
Reference = R1;
ValeurCmp = 10k;
IdModule  = R3;
EndCmp

BeginCmp
TimeStamp = /52405805;
Reference = R2;
ValeurCmp = 10R;
IdModule  = R3;
EndCmp

BeginCmp
TimeStamp = /5240583C;
Reference = R3;
ValeurCmp = 10k;
IdModule  = R3;
EndCmp

BeginCmp
TimeStamp = /52405691;
Reference = R4;
ValeurCmp = 10R;
IdModule  = R3;
EndCmp

BeginCmp
TimeStamp = /52405688;
Reference = R5;
ValeurCmp = 10k;
IdModule  = R3;
EndCmp

BeginCmp
TimeStamp = /5240504D;
Reference = R6;
ValeurCmp = 10k;
IdModule  = R3;
EndCmp

BeginCmp
TimeStamp = /52405054;
Reference = R7;
ValeurCmp = 10k;
IdModule  = R3;
EndCmp

BeginCmp
TimeStamp = /5240505B;
Reference = R8;
ValeurCmp = 10k;
IdModule  = R3;
EndCmp

BeginCmp
TimeStamp = /52404C91;
Reference = R9;
ValeurCmp = 100k;
IdModule  = R3;
EndCmp

BeginCmp
TimeStamp = /52404CC1;
Reference = R10;
ValeurCmp = 100k;
IdModule  = R3;
EndCmp

BeginCmp
TimeStamp = /52404CC6;
Reference = R11;
ValeurCmp = 100k;
IdModule  = R3;
EndCmp

BeginCmp
TimeStamp = /523F03A9;
Reference = R12;
ValeurCmp = 27R;
IdModule  = R3;
EndCmp

BeginCmp
TimeStamp = /523F03B3;
Reference = R13;
ValeurCmp = 27R;
IdModule  = R3;
EndCmp

BeginCmp
TimeStamp = /523F08F6;
Reference = R14;
ValeurCmp = 4k7;
IdModule  = R3;
EndCmp

BeginCmp
TimeStamp = /523F08FA;
Reference = R15;
ValeurCmp = 10k;
IdModule  = R3;
EndCmp

BeginCmp
TimeStamp = /52407913;
Reference = R16;
ValeurCmp = 1k5;
IdModule  = R3;
EndCmp

BeginCmp
TimeStamp = /524077ED;
Reference = R17;
ValeurCmp = 1k5;
IdModule  = R3;
EndCmp

BeginCmp
TimeStamp = /524077F5;
Reference = R18;
ValeurCmp = 1k5;
IdModule  = R3;
EndCmp

BeginCmp
TimeStamp = /5242CB0D;
Reference = R19;
ValeurCmp = 10k;
IdModule  = R3;
EndCmp

BeginCmp
TimeStamp = /5242CAFD;
Reference = R20;
ValeurCmp = 10k;
IdModule  = R3;
EndCmp

BeginCmp
TimeStamp = /523EF219;
Reference = U1;
ValeurCmp = 7805;
IdModule  = TO220_VERT_VREG;
EndCmp

BeginCmp
TimeStamp = /523F0300;
Reference = U2;
ValeurCmp = FT230X;
IdModule  = ssop-16;
EndCmp

BeginCmp
TimeStamp = /523EF233;
Reference = X1;
ValeurCmp = CRYSTAL;
IdModule  = HC-18UV;
EndCmp

EndListe
